**References**

**Seminal Paper**

“Permafrost Tunnel, Camp Tuto, Greenland”, Abel J.F. Jr., Oct. 1960, 19pp, US Army Cold Regions Research and Engineering Laboratory, Technical Report TR73, AD-652712.

The army scientists measured the specific energy of many machines excavating permafrost. By far the most energetically efficient is a man with a pick, thus introducing the concept of *intelligent excavation*.

**A Sampling of Rock Excavation Tools and Methods**

“Hydraulically Actuated Tool for the Mechanical Breaking of Rocks by Means of a Wedge Slidable Through Insert Pieces”, Helmut Darda, U.S. Patent #3,414,328, June 1969. Also, U.S. Patents #3,488,093 Jan. 1970, and #3,995,906 June 1975.

“Study of a Continuous Drill and Blast Tunneling Concept”, March 1973, Rapidex Inc., ARPA order 1579, U.S. Bureau of Mines Contract H0230008, AD-757114.

“Development of a Continuous Drill and Blast Tunneling Concept, Phase II, Final Report”. Carl Peterson, Rapidex Inc., Advanced Research Projects Agency, May 1974,

“Spiral Drill-and-Blast Concept May Speed Up Tunneling Advance Rate”, Peterson CR; Fisk AT; Brooks RE, Mining Engineering Magazine 29(6):29-32, June 1977.

“Rapid Excavation of Rock with Small Charges of High Explosive”, George Clark, Ronald R. Rollins, 18th U.S. Symposium on Rock Mechanics, June 1977.

“Potential Applications of Drill-Split Fragmentation Systems in Underground Mines”, Michael Kaplan and David Chazin, 1979, 188pp, US Bureau of Mines Open File Report 86-80.

“A Novel Concept for a Rock Breaking Machine, Part I, Theoretical Consideration and Model Experiments”, I. Rhyming, G. A. Cooper, and J. Berlie, Proceedings of the Royal Society of London. Series A, Mathematical and Physical Sciences, [Vol. 373, No. 1754 (Dec. 8, 1980)](https://www.jstor.org/stable/i350076), pp. 331-351.

**“**A Novel Concept for a Rock-Breaking Machine, Part II, Excavation Techniques and Experiments at Larger Scale**”,** G. A. Cooper, J. Berlie, and A. Merminod**,** Proceedings of the Royal Society of London. Series A, Mathematical and Physical Sciences, [Vol. 373, No. 1754 (Dec. 8, 1980)](https://www.jstor.org/stable/i350076), pp. 352-372.

“Laboratory Testing of a Radial-Axial Loading Splitting Tool”, Anderson, S. J., and D. E. Swanson, U.S. Bureau of Mines Report of Investigations RI 8722, 1982, 26 pp.

# “Capability Evaluation of the Radial-Axial Splitter”, [Sterling J.](https://stacks.cdc.gov/gsearch?ref=docDetails&name_personal=Anderson%2C%20Sterling%20J.)Anderson and David E. Swanson, U.S. Bureau of Mines [Report of investigations 9091](https://stacks.cdc.gov/gsearch?ref=docDetails&related_series=Report%20of%20investigations%20%28United%20States.%20Bureau%20of%20Mines%29%20).

“Method for Controlled Fragmentation of Hard Rock and Concrete by the Combination Use of Impact Hammers and Small Charge Blasting”, John David Watson and P. Micke, U.S. Patent 5,803,550 Sept. 1998.

“Controlled Fracture Method and Apparatus for Breaking Hard Compact Rock and Concrete Materials”, Chapman Young, U.S. Patent 5,098,163, Mar. 1992.

“Controlled Foam Injection Method and Means for Fragmentation of Hard Compact Rock and Concrete”, Chapman Young, U.S. Patent 6,102,484, Aug. 2000.

“Controlled Foam Injection: a New and Innovative Non-explosive Rock Breaking Technology”, R.G.B. Pickeringand C. Young, [Journal of the Southern African Institute of Mining and Metallurgy](http://www.scielo.org.za/scielo.php?script=sci_serial&pid=2225-6253&lng=en&nrm=iso), Vol.117 n.3 Johannesburg Mar. 2017

Controlled Foam Injection website, Chapman Young, [www.capprex.com](http://www.capprex.com).